Press Release
April 2013

Andreas Behr
Product Owner Sensors
Phone: +49 6151 428 1122
E-Mail: andreas.behr@bkvibro.com

Series ds821 and Series ds822 ATEX - 
A New Generation of Eddy-Current Displacement Sensor Systems 

Brüel & Kjær Vibro, the leading independent supplier of vibration condition monitoring solutions, sets new standards in machine monitoring applications with the launch of a new generation of ECDS systems: Series ds821 and series ds822 ATEX. 

Both systems are available in 5 m and 10 m cable lengths. In previous systems, the selection of the driver unit (oscillators/ demodulators) was contingent on the cable length being used. The new, innovative driver automatically determines the length of the connected cable and adapts the measurement accordingly. The result is increased flexiblity on site and reduced spare part handling while maintaining the quality and accuracy of the measurements.

For more information, please go to http://www.bkvibro.com/en/products/sensors/non-contacting-sensors.html or write to info@bkvibro.com.

17 lines, 796 characters

Company

Brüel & Kjær Vibro is the leading worldwide independent supplier of condition monitoring solutions for rotating machinery. The comprehensive product range comprises vibration sensors (acceleration, velocity and displacement), vibration monitors, handhelds and rack-based plant-wide integrated monitoring solutions. These products plus a suite of comprehensive services fulfil the most demanding applications for safety, condition and performance monitoring of rotating machinery. Monitoring in the power industry is a strategic focus area with numerous applications in the conventional thermal, cogeneration, nuclear, hydro and wind energy sectors.

Based on 50 years of experience and a world-wide sales and support network, Brüel & Kjær Vibro’s monitoring solutions have successfully reduced downtime and maintenance costs and increased machine reliability for our customers world-wide.

Brüel & Kjær Vibro is part of Spectris plc, the leading supplier of productivity enhancing instrumentation and controls.